HemoCue Hb External QC Program

**Directions for performing test:**

* Select the appropriate sample as indicated on the pipette (black solution) and cut off the tip.
* Apply a drop to a hydrophobic surface, e.g. The foil of the inside packaging of the microcuvette
* Fill the microcuvette in one continuous motion, ensuring any excess on the outside is wiped off and that no large bubbles are present. A small bubble along the edge can be ignored.
* Run the external quality control solution as a patient test.
* Test all of your HemoCue Hb meters using the same solution.
* Once analysis is complete, fill out this form and fax to iCCnet on (08) 7117 0635 or email Health.iCCnetSupport@sa.gov.au.

**EQA Number**

|  |  |  |  |
| --- | --- | --- | --- |
|  | **Device Serial Number** | **Result** | **units** |
| **Device 1** |  |  | **g/L** |
| **Device 2** |  |  | **g/L** |

**Date Analysed:**

**Operator:**

**Site Name:**